{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Лист1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Лист1","index":0,"n_rows":33,"n_cols":14,"rows_kept":33,"cut":false,"hidden":false,"merged":[[2,2,2,4],[2,6,2,8],[2,10,2,12]]}
["S4 -S8 Серия Simplex :  Oil Free",null,null,null,null,null,null,null,null,null,null,null,"Курс Euro",{"$f":"NBUCURRENCY(\"EUR\",\"rate\",TODAY())","v":32.328754000000004}]
[]
["Серия S ","Type","S4",null,null,null,"S6",null,null,null,"S8"]
["Максимальное давление, бар","bar",8,null,10,null,8,null,10,null,8,null,10]
["Производительность, м3/ч","m3/h",23.6,null,21.2,null,34.5,null,26,null,53,null,41.3]
["Двигатель IP 55, кВт","kW",4,null,4,null,5.5,null,5.5,null,7.5,null,7.5]
["Регулятор напряжения, Вт","24v",".",null,".",null,".",null,".",null,".",null,"."]
["Акустический корпус",null,".",null,".",null,".",null,".",null,".",null,"."]
["Воздушное охлаждение",null,".",null,".",null,".",null,".",null,".",null,"."]
["Модуль для удаленного мониторинга Mod-Bus-RTU",null,".",null,".",null,".",null,".",null,".",null,"."]
["230 Вт Базовое управление реле"]
["Код",null,"SQ4-30A03",null,"SQ4-30A04",null,"SQ4-30A07",null,"SQ4-30A08",null,"SQ4-30A48",null,"SQ4-30A49"]
["Цена в (Euro)",null,8100,{"$f":"C13*$N$1","v":261862.90740000003},8100,{"$f":"E13*$N$1","v":261862.90740000003},10500,{"$f":"G13*$N$1","v":339451.91700000002},10500,{"$f":"I13*$N$1","v":339451.91700000002},12000,{"$f":"K13*$N$1","v":387945.04800000007},12000,{"$f":"M13*$N$1","v":387945.04800000007}]
["230 Вт Цифровой электронный контроллер HMI"]
["Код",null,"SQ4-30A05",null,"SQ4-30A06",null,"SQ4-30A09",null,"SQ4-30A10",null,"SQ4-30A50",null,"SQ4-30A51"]
["Цена в (Euro) ",null,10100,{"$f":"C16*$N$1","v":326520.41540000006},10100,{"$f":"E16*$N$1","v":326520.41540000006},12500,{"$f":"G16*$N$1","v":404109.42500000005},12500,{"$f":"I16*$N$1","v":404109.42500000005},14000,{"$f":"K16*$N$1","v":452602.55600000004},14000,{"$f":"M16*$N$1","v":452602.55600000004}]
["400 Вт Базовое управление реле"]
["Код",null,"SQ4-30A11",null,"SQ4-30A12",null,"SQ4-30A58",null,"SQ4-30A59",null,"SQ4-30A62",null,"SQ4-30A47"]
["Цена в (Euro)",null,8100,261862.90740000003,8100,261862.90740000003,10500,{"$f":"G19*$N$1","v":339451.91700000002},10500,{"$f":"I19*$N$1","v":339451.91700000002},12000,{"$f":"K19*$N$1","v":387945.04800000007},12000,387945.04800000007]
["400 Вт Цифровой электронный контроллер HMI"]
["Код",null,"SQ4-30A13",null,"SQ4-30A14",null,"SQ4-30A60",null,"SQ4-30A61",null,"SQ4-30A63",null,"SQ4-30A64"]
["Цена в (Euro)",null,10100,326520.41540000006,10100,326520.41540000006,12500,{"$f":"G22*$N$1","v":404109.42500000005},12500,{"$f":"I22*$N$1","v":404109.42500000005},14000,{"$f":"K22*$N$1","v":452602.55600000004},14000,452602.55600000004]
["400 Вт Мягкий старт/ базовое управление реле",null,null,null,null,0]
["Код",null,"NA",null,"NA",null,"SQ4-30A15",null,"SQ4-30A16",null,"SQ4-30A19",null,"SQ4-30A20"]
["Цена в (Euro)",null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},11100,{"$f":"G25*$N$1","v":358849.16940000001},11100,{"$f":"I25*$N$1","v":358849.16940000001},12700,{"$f":"K25*$N$1","v":410575.17580000003},12700,410575.17580000003]
["400 Вт Мягкий старт/ Цифровой электронный контроллер HMI"]
["Код",null,"NA",null,"NA",null,"SQ4-30A17",null,"SQ4-30A18",null,"SQ4-30A21",null,"SQ4-30A22"]
["Цена в (Euro)",null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},13400,{"$f":"G28*$N$1","v":433205.30360000004},13400,{"$f":"I28*$N$1","v":433205.30360000004},14900,{"$f":"K28*$N$1","v":481698.43460000004},14900,481698.43460000004]
[]
["Цены рассчитаны на условиях:"]
["1. Условия поставки - EXW, г. Киев."]
["2. Пусконаладка оборудования не включена."]
["3. Включена стандартная гарантия на оборудование 12 месяцев."]